Electronic Load 1.0 Programmable Constant Current Sink

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - a -

- action : menuItem_t
- ADC_Chan0 : ADCData_t
- ADC_Chan1 : ADCData_t
- ADC_Chan2 : ADCData_t
- ADC_Chan3 : ADCData_t
- ADC_HSTemp : ADCData_t
- ADC_P12 : ADCData_t
- ADC_P5 : ADCData_t
- ADC_Temp : ADCData_t
- ADCCmd : SPI_XmtStruct_t
- ADCDiffVoltsPerLSB : confStruct_t
- ADCHighAmpsPerLSB : confStruct_t
- ADCLowAmpsPerLSB : confStruct_t
- adr : commandTable_t
- array : ADC_RcvStruct_t , ADCData_t , LED_DATA_t , SPI_XmtStruct_t

### - b -

- backlightAlwaysOn : confStruct_t
- backlightOnTime : confStruct_t
- button : control_t

### - c -

- callback : refresh_s
- changeCallback : enterNumber_s
- cmd : commandTable_t
- control : screenItem_t
- curPos : enterNumberVariable_s

### - d -

- DAC : ADC_RcvStruct_t , SPI_XmtStruct_t
- DAC_CMD : ADC_RcvStruct_t , SPI_XmtStruct_t
- dacHighAdj : volatileConfStruct_t
- DACHighAmpsPerLSB : confStruct_t
- DACLowAmpsPerLSB : confStruct_t
- data : ADC_RcvStruct_t , SPI_XmtStruct_t
- ddr : ftestPortsStruct
- dummy : ADC_RcvStruct_t

### - e -

- EnterNumber : control_t
- entry : menu_t

### - f -

- fuse : LED_DATA_t

### - h -

- head : menu_t
- helptext : commandTable_t

### - i -

- i : sinkPrefixValues_t
- i2 : soa_t
- i3 : soa_t
- Ihigh : SPIADCData_t
- Ilow : SPIADCData_t
- iMax : soa_t
- item : screen_t

### - l -

- lastPrefix : prefixValue_t
- LCDBright : confStruct_t
- LCDV0 : confStruct_t
- LED : ADC_RcvStruct_t , SPI_XmtStruct_t

### - m -

- magic : confStruct_t

### - n -

- named : ADC_RcvStruct_t , ADCData_t , LED_DATA_t , SPI_XmtStruct_t
- nPar : text_s
- numberOfItems : screen_t

### - o -

- oldValue : enterNumberVariable_s
- overTemp : LED_DATA_t

### - p -

- p : sinkPrefixValues_t
- P12VoltsPerLSB : confStruct_t
- P5VoltsPerLSB : confStruct_t
- param : enterNumber_s , refresh_s
- pin : ftestPortsStruct
- pMax : soa_t
- port : ftestPortsStruct
- pos : button_s , enterNumber_s , refresh_s , text_s
- powerGreen : LED_DATA_t
- powerRed : LED_DATA_t
- preset : confStruct_t

### - r -

- r : sinkPrefixValues_t
- rangeBlue : LED_DATA_t
- rangeGreen : LED_DATA_t
- rangeHighLimit : volatileConfStruct_t
- rangeLowLimit : volatileConfStruct_t
- RchanP : volatileConfStruct_t
- refresh : control_t
- retval : screenItem_t
- Rhigh : volatileConfStruct_t
- Rlow : volatileConfStruct_t

### - s -

- SBa : volatileConfStruct_t
- SBb : volatileConfStruct_t
- shortcut : menuItem_t
- soa : confStruct_t
- SOA : LED_DATA_t
- spare : LED_DATA_t
- SPIADCData : ADC_RcvStruct_t
- suffix_s : enterNumberVariable_s

### - t -

- tempMax : soa_t
- testMask : ftestPortsStruct
- text : control_t , menuItem_t
- timeout : screen_t
- txtIndex : button_s , text_s
- type : button_s , enterNumber_s , refresh_s , text_s

### - u -

- u : sinkPrefixValues_t

### - v -

- V : SPIADCData_t
- v2 : soa_t
- value : enterNumberVariable_s , prefixValue_t
- var : enterNumber_s
- VImax : volatileConfStruct_t