Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
ADCData_t Union Reference

Holds raw ADC Values for all Channels. More...

## Data Fields
uint16_t | array [8]
| Array for access via Channel Number. More...
struct {
uint16_t ADC_Chan0
uint16_t ADC_Chan1
uint16_t ADC_Chan2
uint16_t ADC_Chan3
uint16_t ADC_HSTemp
| Temperature of the Heatsink. More...
uint16_t ADC_P12
| 12V Supply More...
uint16_t ADC_P5
| 5V Supply More...
uint16_t ADC_Temp
| Display Temperature. More...
} | named
| Named Values per Channel. More...

## Detailed Description

Holds raw ADC Values for all Channels.

## Field Documentation

## ◆ ADC_Chan0

uint16_t ADC_Chan0

## ◆ ADC_Chan1

uint16_t ADC_Chan1

## ◆ ADC_Chan2

uint16_t ADC_Chan2

## ◆ ADC_Chan3

uint16_t ADC_Chan3

## ◆ ADC_HSTemp

uint16_t ADC_HSTemp

Temperature of the Heatsink.

## ◆ ADC_Temp

uint16_t ADC_Temp

Display Temperature.

## ◆ ADC_P5

uint16_t ADC_P5

5V Supply

## ◆ ADC_P12

uint16_t ADC_P12

12V Supply

## ◆ named

struct { ... } named

Named Values per Channel.

## ◆ array

uint16_t array[8]

Array for access via Channel Number.

The documentation for this union was generated from the following file:

- adc.h