Electronic Load 1.0 Programmable Constant Current Sink

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- saveval : control.c
- scancnt : keyboard.c , keyboard.h
- scanKeyboard() : keyboard.h
- scanRotaryEncoder() : keyboard.h
- Screen() : screen.c , screen.h
- screenDischgTest : screen.c
- screenManualTest : screen.c
- screenTimeout_t : screen.h
- screenVersion : screen.c , screen.h
- secCnt : Eload.c , Eload.h
- SetHighCurrentMode() : spi.h , spi.c
- SetLowCurrentMode() : spi.c , spi.h
- SetOvertempError() : led.h
- SetSOAError() : led.h
- SFLAG_REFRESH : Eload.h
- sFlags : Eload.h , screen.c
- sinkPVal : screen.c
- SOA_I2 : config.h
- SOA_I3 : config.h
- SOA_IMAX : config.h
- SOA_PMAX : config.h
- SOA_V2 : config.h
- SOAGetImax() : config.c , config.h
- soaIMaxLUT : spi.c , spi.h
- SoaLimit() : spi.c
- SPIADCAvg : spi.c , spi.h
- SPIADCBusy() : spi.h
- SPIADCVOLTSPERLSB : config.h
- SPIDeselectADC() : spi.h
- SPIDeselectDAC() : spi.h
- SPIDIFFVOLTSPERLSB : config.h
- SpiGetADC() : spi.h
- SpiGetADC2() : spi.h
- SPIHIGHAMPSPERLSB : config.h
- SPIInit() : spi.c , spi.h
- SPILOWAMPSPERLSB : config.h
- SPIPtr : spi.c
- SpiSelectADC() : spi.h
- SpiSelectDAC() : spi.h
- SpiSendAndReceiveByte() : spi.h , spi.c
- SPISendData : spi.c
- SPISetLEDs() : spi.h , spi.c
- SPIVREF : config.h
- START : control.h
- SWUnregFromADC() : sensors.h