<map id="DrawTempCallback" name="DrawTempCallback">
<area shape="rect" id="node1" title=" " alt="" coords="5,31,139,57"/>
<area shape="rect" id="node2" href="$sensors_8c.html#a25ac5c6f9d5812eca2a3f84401825dec" title="Converts the ADC&#45;Temp of the Display NTC Value to Celsius This function also calculates the derating ..." alt="" coords="196,5,307,32"/>
<area shape="rect" id="node4" href="$sensors_8c.html#a431ae2d9b1840dcb23cd8a8a08c27a3e" title="Converts the ADC&#45;Temp Value of the Heat Sink NTC to Celsius." alt="" coords="187,56,316,83"/>
<area shape="rect" id="node3" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="386,5,481,32"/>
<area shape="rect" id="node5" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="386,56,481,83"/>
<area shape="rect" id="node8" href="$led_8h.html#a449e7c96d56eafe4856d89eaafb20583" title="Sets the Overtemp Error Flag and the LED." alt="" coords="371,107,496,133"/>
<area shape="rect" id="node9" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="364,157,503,184"/>
<area shape="rect" id="node6" href="$spi_8c.html#a0e0bc8d4968cb844619c63ac93da1e4e" title="The same as DACSetRaw() but without updating the controls This function has been introduced to allow ..." alt="" coords="551,31,671,57"/>
<area shape="rect" id="node7" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="574,81,647,108"/>
</map>
