Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
soa_t Struct Reference

## Data Fields
double | i2
| Current Limit for Pv-Area (3.5A for TIP102) More...
double | i3
| Current Limit for 60V (350mA for TIP102) More...
double | iMax
| The absolute maximum Current. Eload will not allow currents more than this. More...
double | pMax
| Up to this Voltage, 4A are allowable (20V for TIP102) More...
uint8_t | tempMax
double | v2
| Voltage Limit for Pv-Area (25V for TIP102) More...

## Field Documentation

## ◆ tempMax

uint8_t tempMax

## ◆ pMax

double pMax

Up to this Voltage, 4A are allowable (20V for TIP102)

## ◆ v2

double v2

Voltage Limit for Pv-Area (25V for TIP102)

## ◆ iMax

double iMax

The absolute maximum Current. Eload will not allow currents more than this.

## ◆ i2

double i2

Current Limit for Pv-Area (3.5A for TIP102)

## ◆ i3

double i3

Current Limit for 60V (350mA for TIP102)

The documentation for this struct was generated from the following file:

- config.h