ElectronicLoad 1.0 Programmable Constant Current Sink

- Main Page
- Related Pages
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Pages
Data Fields
refresh_t Struct Reference

Variables for an auto-refresh-control. More...

## Data Fields
void(* | callback )(uint8_t param)
| Callback function which has to draw the value. More...
uint8_t | param
| Parameter for the callback function. More...
const controlType_t | type
uint8_t | x
| X-Position. More...
uint8_t | y
| Y-Position. More...

## Detailed Description

Variables for an auto-refresh-control.

The structure provides a callback function which has to draw the value. It will be called in regular intervals to actualize its content.

## Field Documentation

void(* callback)(uint8_t param)

Callback function which has to draw the value.

uint8_t param

Parameter for the callback function.

const controlType_t type

uint8_t x

X-Position.

uint8_t y

Y-Position.

The documentation for this struct was generated from the following file:

- control.h