<map id="Menu" name="Menu">
<area shape="rect" id="node1" title="Executes a menu page." alt="" coords="5,259,60,285"/>
<area shape="rect" id="node2" href="$lcd_8c.html#a3a94c0f44f76db891e66d98966f904e8" title="Clears the LCD and sets Cursor to Home Postion." alt="" coords="332,5,409,32"/>
<area shape="rect" id="node10" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="898,385,971,412"/>
<area shape="rect" id="node11" href="$menu_8c.html#aaf8d6b4726fb1980061d081c2c005afb" title="Draws a menu page (without erasing the display before)" alt="" coords="142,107,225,133"/>
<area shape="rect" id="node16" href="$keyboard_8c.html#a05e82dd654fd4e6c001ef94fcacc1f91" title="Gets the next key from the keyboard buffer." alt="" coords="150,259,217,285"/>
<area shape="rect" id="node17" href="$_eload_8c.html#a51bdf9afc51ba51479247b238d86d5fe" title="Process Communication&#45;, Time&#45; and Key&#45;Flags." alt="" coords="148,309,219,336"/>
<area shape="rect" id="node45" href="$spi_8c.html#ae7d52bffdf79197de02b2064e0615c88" title="Sets the DAC to a certain Current." alt="" coords="507,1272,609,1299"/>
<area shape="rect" id="node50" href="$control_8c.html#a559e0112d069cc4850222e6c541cca50" title="Sets the Value." alt="" coords="108,841,259,868"/>
<area shape="rect" id="node3" href="$lcd_8c.html#a66337720cc00454cf4d5b4c59d210708" title="Writes a Command&#45;Byte to the Display." alt="" coords="701,56,807,83"/>
<area shape="rect" id="node4" href="$lcd_8c.html#a8bbe315df5131e3567cf5960938c77e5" title="Waits until the LCD is ready." alt="" coords="897,81,972,108"/>
<area shape="rect" id="node8" href="$lcd_8c.html#afd5485a731dca173a51b8270c24404e2" title="Writes a Byte to the Display." alt="" coords="895,19,974,45"/>
<area shape="rect" id="node5" href="$lcd_8c.html#af1559a17726b03016098580e375d749e" title=" " alt="" coords="1048,81,1152,108"/>
<area shape="rect" id="node6" href="$lcd_8c.html#a691499026cdf181d4b30b4e42ff2f110" title="Reads a Byte from the LCD." alt="" coords="1205,81,1283,108"/>
<area shape="rect" id="node7" href="$lcd_8c.html#a9a49d41e6b1bc64016ca9adbb8f7ab89" title="Reads a nibble from LCD." alt="" coords="1331,81,1444,108"/>
<area shape="rect" id="node9" href="$lcd_8c.html#a1c6b194d0b91174b01ae5fed203241f5" title="Writes a nibble to the LCD." alt="" coords="1043,19,1157,45"/>
<area shape="rect" id="node12" href="$lcd_8c.html#a3d6576a7f684f5764f35c778588248cc" title="Sets the Cursor Position." alt="" coords="323,157,418,184"/>
<area shape="rect" id="node14" href="$lcd_8c.html#a3880fc70c04a78c0bbae2e88f2445d44" title="Displays a String in Flash Memory." alt="" coords="307,56,435,83"/>
<area shape="rect" id="node15" href="$lcd_8c.html#a287340ff1ccf756cd9668d289ba8ce23" title="Writes a Data&#45;Byte to the Display." alt="" coords="505,68,611,95"/>
<area shape="rect" id="node13" href="$lcd_8c.html#ab8300df8f51fbc77b8895257c2a8085f" title="Sets the Cursor Position." alt="" coords="519,144,597,171"/>
<area shape="rect" id="node18" href="$_eload_8c.html#aefd1a6765377077adfbbf8ddda17e264" title="Checks for Communication Flags." alt="" coords="521,309,595,336"/>
<area shape="rect" id="node21" href="$_eload_8c.html#af35578a7ae9d130357ffc9be42ed864d" title="Checks for Time Flags." alt="" coords="335,740,407,767"/>
<area shape="rect" id="node19" href="$usartcmd_8c.html#aae6978a287d0ea7d42f3e5d1b496ce63" title="Executes one command line." alt="" coords="699,360,809,387"/>
<area shape="rect" id="node20" href="$uart_8h.html#a31900f4f13bc5468a0d1533b6bbbd9ac" title="Asserts RTS to the Host Line, i.e. allows the Host to send Data." alt="" coords="711,309,797,336"/>
<area shape="rect" id="node22" href="$spi_8c.html#a554eba0a42a9236e1069c8478a9142fa" title="Returns the Life Value for the Current." alt="" coords="487,715,629,741"/>
<area shape="rect" id="node23" href="$spi_8c.html#a9c64a243c6b576aee998df37c8a2f1a1" title="Returns the Life Value for the Current." alt="" coords="489,765,627,792"/>
<area shape="rect" id="node24" href="$spi_8c.html#a6f60819b713ab284521b04a3909b532e" title="Returns the Life Value for the Sink Voltage." alt="" coords="496,816,620,843"/>
<area shape="rect" id="node25" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="688,968,820,995"/>
<area shape="rect" id="node26" href="$spi_8c.html#a80a3e7ab4fc8126893d20222ce18f7ec" title="Returns the averaged Value for the Current." alt="" coords="681,689,827,716"/>
<area shape="rect" id="node27" href="$spi_8c.html#acb3eafeb13b87ee2d275605d543c372c" title="Returns the averaged Value for the Current." alt="" coords="683,892,825,919"/>
<area shape="rect" id="node28" href="$spi_8c.html#ab815264416b8e8438b2910c13a010d0f" title="Returns the averaged Value for the Sink Voltage." alt="" coords="495,1019,621,1045"/>
<area shape="rect" id="node29" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="707,1069,801,1096"/>
<area shape="rect" id="node30" href="$sensors_8c.html#a1bd30a33d99acf39dc419dfcda84a12b" title="Converts a Unreg&#45;Raw ADC Value to Voltage." alt="" coords="507,1120,609,1147"/>
<area shape="rect" id="node31" href="$sensors_8c.html#a25ac5c6f9d5812eca2a3f84401825dec" title="Converts the ADC&#45;Temp of the Display NTC Value to Celsius This function also calculates the derating ..." alt="" coords="503,1171,613,1197"/>
<area shape="rect" id="node32" href="$sensors_8c.html#a431ae2d9b1840dcb23cd8a8a08c27a3e" title="Converts the ADC&#45;Temp Value of the Heat Sink NTC to Celsius." alt="" coords="493,1221,623,1248"/>
<area shape="rect" id="node37" href="$_eload_8c.html#a220ba0eebf40921c1536740d305103f3" title=" " alt="" coords="513,360,603,387"/>
<area shape="rect" id="node38" href="$spi_8c.html#ad26ad99ad32438be4c880123c08d8ede" title="Returns the Current for a given Value." alt="" coords="700,512,808,539"/>
<area shape="rect" id="node39" href="$spi_8c.html#a8fb1a7434a0afa308a1e334c16867f68" title="Gets the Ampere Seconds consumed." alt="" coords="515,461,601,488"/>
<area shape="rect" id="node40" href="$adc_8h.html#a3b504b59dfbdde96a7a6762da16e1a93" title="Resets the Min/Max values of the Analog Values." alt="" coords="493,512,623,539"/>
<area shape="rect" id="node41" href="$spi_8c.html#a8508d5d475a25c17630a31548c739e17" title=" " alt="" coords="506,867,610,893"/>
<area shape="rect" id="node42" href="$lcd_8c.html#a76e163e293ed77d6cecdcadc800d20a7" title="Has to be called once per Second by the surrounding program." alt="" coords="483,613,633,640"/>
<area shape="rect" id="node33" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="707,1221,801,1248"/>
<area shape="rect" id="node35" href="$led_8h.html#a449e7c96d56eafe4856d89eaafb20583" title="Sets the Overtemp Error Flag and the LED." alt="" coords="691,1120,817,1147"/>
<area shape="rect" id="node36" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="685,1171,823,1197"/>
<area shape="rect" id="node34" href="$spi_8c.html#a0e0bc8d4968cb844619c63ac93da1e4e" title="The same as DACSetRaw() but without updating the controls This function has been introduced to allow ..." alt="" coords="875,1221,995,1248"/>
<area shape="rect" id="node43" href="$lcd_8h.html#ade0a120b714ecbdb9a6903ab8cc0287c" title="Gets the current Brightness of the LCD Backlight." alt="" coords="689,639,819,665"/>
<area shape="rect" id="node44" href="$lcd_8h.html#afa35e4a61570e2824382729f139fc5be" title="Sets the Brightness of the LCD Backlight." alt="" coords="689,588,819,615"/>
<area shape="rect" id="node46" href="$led_8h.html#afa870201459ed745a0dffe22327ae35f" title="Clears the Overtemp Error Flag and the LED." alt="" coords="687,1424,821,1451"/>
<area shape="rect" id="node47" href="$led_8h.html#aea553a9b3a4abb12927063350a84a44e" title="Sets the SOA Error Flag and the LED." alt="" coords="705,1272,803,1299"/>
<area shape="rect" id="node48" href="$led_8h.html#a26641dea186ec8ea453761150787698f" title="Clears the SOA Error Flag and the LED." alt="" coords="700,1323,808,1349"/>
<area shape="rect" id="node49" href="$spi_8c.html#a6bb86d3005dc9addb4b5695add9e26e4" title="Sets High Current Mode." alt="" coords="683,1373,825,1400"/>
</map>
