<map id="HSTempFromADC" name="HSTempFromADC">
<area shape="rect" id="node1" title="Converts the ADC&#45;Temp Value of the Heat Sink NTC to Celsius." alt="" coords="5,81,135,108"/>
<area shape="rect" id="node2" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="205,5,299,32"/>
<area shape="rect" id="node3" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="205,56,299,83"/>
<area shape="rect" id="node6" href="$led_8h.html#a449e7c96d56eafe4856d89eaafb20583" title="Sets the Overtemp Error Flag and the LED." alt="" coords="189,107,315,133"/>
<area shape="rect" id="node7" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="183,157,321,184"/>
<area shape="rect" id="node4" href="$spi_8c.html#a0e0bc8d4968cb844619c63ac93da1e4e" title="The same as DACSetRaw() but without updating the controls This function has been introduced to allow ..." alt="" coords="369,31,489,57"/>
<area shape="rect" id="node5" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="393,81,466,108"/>
</map>
