ElectronicLoad 1.0 An ultrasonic Level Meter for Stormwater Cisterns

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros
Data Fields
signalOutput_t Struct Reference

Holds the Thresholds for a Signal Optocoupler Output. More...

## Data Fields
uint16_t | activeAbove
| Threshold above this the output is active. More...
uint16_t | activeBelow
| Threshold below this the output is active. More...

## Detailed Description

Holds the Thresholds for a Signal Optocoupler Output.

## Field Documentation

uint16_t activeAbove

Threshold above this the output is active.

uint16_t activeBelow

Threshold below this the output is active.

The documentation for this struct was generated from the following file:

- config.h