Electronic Load 1.0 Programmable Constant Current Sink

delay.h
Go to the documentation of this file.
1
13 #ifndef DELAY_H_
14 #define DELAY_H_
15
16
17 extern void delay50us(void);
18 extern void delay5ms(void);
19 extern void delay50ms(void);
20 extern void delay1s(void);
21
22
23
24
25 #endif /* DELAY_H_ */
delay50ms
void delay50ms(void)
Delays for 50ms. This routine is hard-timed and does not rely on interrupts.
delay50us
void delay50us(void)
Delays for 50us. This routine is hard-timed and does not rely on interrupts.
delay5ms
void delay5ms(void)
Delays for 5ms. This routine is hard-timed and does not rely on interrupts.
delay1s
void delay1s(void)
Delays for one second. This routine is hard-timed and does not rely on interrupts.