<map id="doScreenDischgTest" name="doScreenDischgTest">
<area shape="rect" id="node1" title=" " alt="" coords="5,385,148,412"/>
<area shape="rect" id="node2" href="$screen_8c.html#afb7451f925f996735c48ee98b05c9ecf" title="Handles a screen." alt="" coords="196,385,259,412"/>
<area shape="rect" id="node3" href="$lcd_8c.html#a3a94c0f44f76db891e66d98966f904e8" title="Clears the LCD and sets Cursor to Home Postion." alt="" coords="563,259,640,285"/>
<area shape="rect" id="node7" href="$screen_8c.html#a57d1ff74a6ed272c3188f7c771c48737" title="(Re&#45;) draws a control" alt="" coords="555,81,647,108"/>
<area shape="rect" id="node8" href="$lcd_8c.html#ab8300df8f51fbc77b8895257c2a8085f" title="Sets the Cursor Position." alt="" coords="1141,183,1219,209"/>
<area shape="rect" id="node11" href="$control_8c.html#acc188afe436740b989d73613cfa1e2cb" title="Enter a Number via Keyboard and/or Encoder." alt="" coords="763,259,862,285"/>
<area shape="rect" id="node13" href="$keyboard_8c.html#a05e82dd654fd4e6c001ef94fcacc1f91" title="Gets the next key from the keyboard buffer." alt="" coords="975,309,1042,336"/>
<area shape="rect" id="node15" href="$screen_8c.html#ade4af775d47e7a21b42ac7cb8685c3a7" title="Redraws all Auto&#45;Refresh items." alt="" coords="323,107,449,133"/>
<area shape="rect" id="node16" href="$_eload_8c.html#a51bdf9afc51ba51479247b238d86d5fe" title="Process Communication&#45;, Time&#45; and Key&#45;Flags." alt="" coords="351,461,421,488"/>
<area shape="rect" id="node40" href="$control_8c.html#a7ff3148353eb1bf46218aa8adfeb1439" title="Saves the Value of the Input Field Purpose is to reset it to the original value when the user exits t..." alt="" coords="307,411,465,437"/>
<area shape="rect" id="node41" href="$lcd_8c.html#ab8dcdcda55348d1e94865935d68493bf" title=" " alt="" coords="550,1145,653,1172"/>
<area shape="rect" id="node42" href="$keyboard_8h.html#acfb6a1aaeae6386a5fc554a48b4c17ba" title="Returns True if Keystrokes are pending." alt="" coords="353,512,419,539"/>
<area shape="rect" id="node43" href="$lcd_8c.html#a9d99627e6f7fe5fcb487322471b7b5b1" title=" " alt="" coords="1129,1424,1231,1451"/>
<area shape="rect" id="node44" href="$control_8c.html#a76d20196a2d85e27ca96c59f84127abc" title="Restores the old Value of the Input Field Purpose is to reset it to the original value when the user ..." alt="" coords="513,208,689,235"/>
<area shape="rect" id="node45" href="$spi_8c.html#ae7d52bffdf79197de02b2064e0615c88" title="Sets the DAC to a certain Current." alt="" coords="761,1475,864,1501"/>
<area shape="rect" id="node50" href="$control_8c.html#a559e0112d069cc4850222e6c541cca50" title="Sets the Value." alt="" coords="311,1525,461,1552"/>
<area shape="rect" id="node4" href="$lcd_8c.html#a66337720cc00454cf4d5b4c59d210708" title="Writes a Command&#45;Byte to the Display." alt="" coords="1279,259,1384,285"/>
<area shape="rect" id="node5" href="$lcd_8c.html#a8bbe315df5131e3567cf5960938c77e5" title="Waits until the LCD is ready." alt="" coords="1434,95,1509,121"/>
<area shape="rect" id="node6" href="$lcd_8c.html#afd5485a731dca173a51b8270c24404e2" title="Writes a Byte to the Display." alt="" coords="1432,183,1511,209"/>
<area shape="rect" id="node9" href="$lcd_8c.html#a287340ff1ccf756cd9668d289ba8ce23" title="Writes a Data&#45;Byte to the Display." alt="" coords="1279,76,1384,103"/>
<area shape="rect" id="node10" href="$lcd_8c.html#a3880fc70c04a78c0bbae2e88f2445d44" title="Displays a String in Flash Memory." alt="" coords="749,5,877,32"/>
<area shape="rect" id="node12" href="$control_8c.html#a3447000f6d8fff3d9310f8575ea9c963" title="Draws the Input Field." alt="" coords="945,208,1072,235"/>
<area shape="rect" id="node14" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="1143,563,1217,589"/>
<area shape="rect" id="node17" href="$_eload_8c.html#aefd1a6765377077adfbbf8ddda17e264" title="Checks for Communication Flags." alt="" coords="775,411,850,437"/>
<area shape="rect" id="node20" href="$_eload_8c.html#af35578a7ae9d130357ffc9be42ed864d" title="Checks for Time Flags." alt="" coords="565,867,637,893"/>
<area shape="rect" id="node18" href="$usartcmd_8c.html#aae6978a287d0ea7d42f3e5d1b496ce63" title="Executes one command line." alt="" coords="953,512,1064,539"/>
<area shape="rect" id="node19" href="$uart_8h.html#a31900f4f13bc5468a0d1533b6bbbd9ac" title="Asserts RTS to the Host Line, i.e. allows the Host to send Data." alt="" coords="966,461,1051,488"/>
<area shape="rect" id="node21" href="$spi_8c.html#a554eba0a42a9236e1069c8478a9142fa" title="Returns the Life Value for the Current." alt="" coords="741,664,884,691"/>
<area shape="rect" id="node22" href="$spi_8c.html#a9c64a243c6b576aee998df37c8a2f1a1" title="Returns the Life Value for the Current." alt="" coords="744,715,881,741"/>
<area shape="rect" id="node23" href="$spi_8c.html#a6f60819b713ab284521b04a3909b532e" title="Returns the Life Value for the Sink Voltage." alt="" coords="751,765,875,792"/>
<area shape="rect" id="node24" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="943,867,1075,893"/>
<area shape="rect" id="node25" href="$spi_8c.html#a80a3e7ab4fc8126893d20222ce18f7ec" title="Returns the averaged Value for the Current." alt="" coords="936,563,1081,589"/>
<area shape="rect" id="node26" href="$spi_8c.html#acb3eafeb13b87ee2d275605d543c372c" title="Returns the averaged Value for the Current." alt="" coords="937,740,1080,767"/>
<area shape="rect" id="node27" href="$spi_8c.html#ab815264416b8e8438b2910c13a010d0f" title="Returns the averaged Value for the Sink Voltage." alt="" coords="750,1019,875,1045"/>
<area shape="rect" id="node28" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="961,1005,1056,1032"/>
<area shape="rect" id="node29" href="$sensors_8c.html#a1bd30a33d99acf39dc419dfcda84a12b" title="Converts a Unreg&#45;Raw ADC Value to Voltage." alt="" coords="761,1120,864,1147"/>
<area shape="rect" id="node30" href="$sensors_8c.html#a25ac5c6f9d5812eca2a3f84401825dec" title="Converts the ADC&#45;Temp of the Display NTC Value to Celsius This function also calculates the derating ..." alt="" coords="757,1069,868,1096"/>
<area shape="rect" id="node31" href="$sensors_8c.html#a431ae2d9b1840dcb23cd8a8a08c27a3e" title="Converts the ADC&#45;Temp Value of the Heat Sink NTC to Celsius." alt="" coords="748,968,877,995"/>
<area shape="rect" id="node34" href="$_eload_8c.html#a220ba0eebf40921c1536740d305103f3" title=" " alt="" coords="768,1272,857,1299"/>
<area shape="rect" id="node35" href="$spi_8c.html#ad26ad99ad32438be4c880123c08d8ede" title="Returns the Current for a given Value." alt="" coords="955,1272,1063,1299"/>
<area shape="rect" id="node36" href="$spi_8c.html#a8fb1a7434a0afa308a1e334c16867f68" title="Gets the Ampere Seconds consumed." alt="" coords="769,1221,856,1248"/>
<area shape="rect" id="node37" href="$adc_8h.html#a3b504b59dfbdde96a7a6762da16e1a93" title="Resets the Min/Max values of the Analog Values." alt="" coords="748,512,877,539"/>
<area shape="rect" id="node38" href="$spi_8c.html#a8508d5d475a25c17630a31548c739e17" title=" " alt="" coords="761,613,865,640"/>
<area shape="rect" id="node39" href="$lcd_8c.html#a76e163e293ed77d6cecdcadc800d20a7" title="Has to be called once per Second by the surrounding program." alt="" coords="737,563,888,589"/>
<area shape="rect" id="node32" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="961,1056,1056,1083"/>
<area shape="rect" id="node33" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="939,1183,1078,1209"/>
<area shape="rect" id="node46" href="$led_8h.html#afa870201459ed745a0dffe22327ae35f" title="Clears the Overtemp Error Flag and the LED." alt="" coords="941,1475,1076,1501"/>
<area shape="rect" id="node47" href="$led_8h.html#aea553a9b3a4abb12927063350a84a44e" title="Sets the SOA Error Flag and the LED." alt="" coords="959,1525,1058,1552"/>
<area shape="rect" id="node48" href="$led_8h.html#a26641dea186ec8ea453761150787698f" title="Clears the SOA Error Flag and the LED." alt="" coords="955,1576,1063,1603"/>
<area shape="rect" id="node49" href="$spi_8c.html#a6bb86d3005dc9addb4b5695add9e26e4" title="Sets High Current Mode." alt="" coords="937,1627,1080,1653"/>
</map>
