Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
LED_DATA_t Union Reference

## Data Fields
LED_FLASH_t | array [8]
struct {
LED_FLASH_t fuse
LED_FLASH_t overTemp
LED_FLASH_t powerGreen
LED_FLASH_t powerRed
LED_FLASH_t rangeBlue
LED_FLASH_t rangeGreen
LED_FLASH_t SOA
LED_FLASH_t spare
} | named

## Field Documentation

## ◆ powerGreen

LED_FLASH_t powerGreen

## ◆ powerRed

LED_FLASH_t powerRed

## ◆ rangeGreen

LED_FLASH_t rangeGreen

## ◆ rangeBlue

LED_FLASH_t rangeBlue

## ◆ overTemp

LED_FLASH_t overTemp

## ◆ SOA

LED_FLASH_t SOA

## ◆ fuse

LED_FLASH_t fuse

## ◆ spare

LED_FLASH_t spare

## ◆ named

struct { ... } named

## ◆ array

LED_FLASH_t array[8]

The documentation for this union was generated from the following file:

- led.h