<map id="ReadConfig" name="ReadConfig">
<area shape="rect" id="node1" title="Reads the Config&#45;Struct from EEPROM into config." alt="" coords="5,56,93,83"/>
<area shape="rect" id="node2" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="485,5,559,32"/>
<area shape="rect" id="node3" href="$config_8c.html#a2c4fb1d41048956f14186db4f53bfdca" title="Loads default config values into conf&#45;struct and stores it in non volatile Memory." alt="" coords="167,56,265,83"/>
<area shape="rect" id="node6" href="$spi_8c.html#a0ee44263f025b4578806ba136aa79edc" title="Calculates the Lookup Table for IMax." alt="" coords="141,132,291,159"/>
<area shape="rect" id="node4" href="$delay_8h.html#a32bb3007d169096acb7198ce4d0be5d2" title="Delays for one second. This routine is hard&#45;timed and does not rely on interrupts." alt="" coords="355,56,421,83"/>
<area shape="rect" id="node5" href="$config_8c.html#ab82705424ddc91b0a7d3c5fa8420640d" title="Writes the Config&#45;Struct to EEPROM." alt="" coords="343,107,433,133"/>
<area shape="rect" id="node7" href="$config_8c.html#a9bc129fa4052524d8c68e0c1b578a10e" title="Calculate maximum allowable Current at a given Voltage." alt="" coords="339,157,437,184"/>
</map>
