<map id="Screen" name="Screen">
<area shape="rect" id="node1" title="Handles a screen." alt="" coords="5,418,68,445"/>
<area shape="rect" id="node2" href="$lcd_8c.html#a3a94c0f44f76db891e66d98966f904e8" title="Clears the LCD and sets Cursor to Home Postion." alt="" coords="372,38,449,65"/>
<area shape="rect" id="node6" href="$screen_8c.html#a57d1ff74a6ed272c3188f7c771c48737" title="(Re&#45;) draws a control" alt="" coords="365,317,457,343"/>
<area shape="rect" id="node7" href="$lcd_8c.html#ab8300df8f51fbc77b8895257c2a8085f" title="Sets the Cursor Position." alt="" coords="963,227,1042,254"/>
<area shape="rect" id="node10" href="$control_8c.html#acc188afe436740b989d73613cfa1e2cb" title="Enter a Number via Keyboard and/or Encoder." alt="" coords="573,443,671,470"/>
<area shape="rect" id="node13" href="$keyboard_8c.html#a05e82dd654fd4e6c001ef94fcacc1f91" title="Gets the next key from the keyboard buffer." alt="" coords="785,494,851,521"/>
<area shape="rect" id="node15" href="$screen_8c.html#ade4af775d47e7a21b42ac7cb8685c3a7" title="Redraws all Auto&#45;Refresh items." alt="" coords="133,342,258,369"/>
<area shape="rect" id="node16" href="$_eload_8c.html#a51bdf9afc51ba51479247b238d86d5fe" title="Process Communication&#45;, Time&#45; and Key&#45;Flags." alt="" coords="160,545,231,571"/>
<area shape="rect" id="node40" href="$control_8c.html#a7ff3148353eb1bf46218aa8adfeb1439" title="Saves the Value of the Input Field Purpose is to reset it to the original value when the user exits t..." alt="" coords="116,835,275,862"/>
<area shape="rect" id="node41" href="$lcd_8c.html#ab8dcdcda55348d1e94865935d68493bf" title=" " alt="" coords="951,89,1054,115"/>
<area shape="rect" id="node42" href="$keyboard_8h.html#acfb6a1aaeae6386a5fc554a48b4c17ba" title="Returns True if Keystrokes are pending." alt="" coords="162,886,229,913"/>
<area shape="rect" id="node43" href="$lcd_8c.html#a9d99627e6f7fe5fcb487322471b7b5b1" title=" " alt="" coords="360,139,461,166"/>
<area shape="rect" id="node44" href="$control_8c.html#a76d20196a2d85e27ca96c59f84127abc" title="Restores the old Value of the Input Field Purpose is to reset it to the original value when the user ..." alt="" coords="323,393,499,419"/>
<area shape="rect" id="node45" href="$spi_8c.html#ae7d52bffdf79197de02b2064e0615c88" title="Sets the DAC to a certain Current." alt="" coords="571,1533,673,1559"/>
<area shape="rect" id="node50" href="$control_8c.html#a559e0112d069cc4850222e6c541cca50" title="Sets the Value." alt="" coords="120,937,271,963"/>
<area shape="rect" id="node3" href="$lcd_8c.html#a66337720cc00454cf4d5b4c59d210708" title="Writes a Command&#45;Byte to the Display." alt="" coords="1115,215,1220,242"/>
<area shape="rect" id="node4" href="$lcd_8c.html#a8bbe315df5131e3567cf5960938c77e5" title="Waits until the LCD is ready." alt="" coords="1270,222,1345,249"/>
<area shape="rect" id="node5" href="$lcd_8c.html#afd5485a731dca173a51b8270c24404e2" title="Writes a Byte to the Display." alt="" coords="1268,279,1347,306"/>
<area shape="rect" id="node8" href="$lcd_8c.html#a287340ff1ccf756cd9668d289ba8ce23" title="Writes a Data&#45;Byte to the Display." alt="" coords="1115,291,1220,318"/>
<area shape="rect" id="node9" href="$lcd_8c.html#a3880fc70c04a78c0bbae2e88f2445d44" title="Displays a String in Flash Memory." alt="" coords="939,342,1067,369"/>
<area shape="rect" id="node11" href="$control_8c.html#a3447000f6d8fff3d9310f8575ea9c963" title="Draws the Input Field." alt="" coords="755,393,881,419"/>
<area shape="rect" id="node14" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="966,722,1039,749"/>
<area shape="rect" id="node12" href="$lcd_8c.html#af90e3b9dd751560aaa5e743ad2a7e17c" title="Displays a String." alt="" coords="947,393,1059,419"/>
<area shape="rect" id="node17" href="$_eload_8c.html#aefd1a6765377077adfbbf8ddda17e264" title="Checks for Communication Flags." alt="" coords="585,545,659,571"/>
<area shape="rect" id="node20" href="$_eload_8c.html#af35578a7ae9d130357ffc9be42ed864d" title="Checks for Time Flags." alt="" coords="375,925,447,951"/>
<area shape="rect" id="node18" href="$usartcmd_8c.html#aae6978a287d0ea7d42f3e5d1b496ce63" title="Executes one command line." alt="" coords="763,545,873,571"/>
<area shape="rect" id="node19" href="$uart_8h.html#a31900f4f13bc5468a0d1533b6bbbd9ac" title="Asserts RTS to the Host Line, i.e. allows the Host to send Data." alt="" coords="775,646,861,673"/>
<area shape="rect" id="node21" href="$spi_8c.html#a554eba0a42a9236e1069c8478a9142fa" title="Returns the Life Value for the Current." alt="" coords="551,1203,693,1230"/>
<area shape="rect" id="node22" href="$spi_8c.html#a9c64a243c6b576aee998df37c8a2f1a1" title="Returns the Life Value for the Current." alt="" coords="553,1254,691,1281"/>
<area shape="rect" id="node23" href="$spi_8c.html#a6f60819b713ab284521b04a3909b532e" title="Returns the Life Value for the Sink Voltage." alt="" coords="560,1305,684,1331"/>
<area shape="rect" id="node24" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="752,950,884,977"/>
<area shape="rect" id="node25" href="$spi_8c.html#a80a3e7ab4fc8126893d20222ce18f7ec" title="Returns the averaged Value for the Current." alt="" coords="745,899,891,926"/>
<area shape="rect" id="node26" href="$spi_8c.html#acb3eafeb13b87ee2d275605d543c372c" title="Returns the averaged Value for the Current." alt="" coords="747,798,889,825"/>
<area shape="rect" id="node27" href="$spi_8c.html#ab815264416b8e8438b2910c13a010d0f" title="Returns the averaged Value for the Sink Voltage." alt="" coords="559,697,685,723"/>
<area shape="rect" id="node28" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="771,1355,865,1382"/>
<area shape="rect" id="node29" href="$sensors_8c.html#a1bd30a33d99acf39dc419dfcda84a12b" title="Converts a Unreg&#45;Raw ADC Value to Voltage." alt="" coords="571,747,673,774"/>
<area shape="rect" id="node30" href="$sensors_8c.html#a25ac5c6f9d5812eca2a3f84401825dec" title="Converts the ADC&#45;Temp of the Display NTC Value to Celsius This function also calculates the derating ..." alt="" coords="567,1355,677,1382"/>
<area shape="rect" id="node31" href="$sensors_8c.html#a431ae2d9b1840dcb23cd8a8a08c27a3e" title="Converts the ADC&#45;Temp Value of the Heat Sink NTC to Celsius." alt="" coords="557,1457,687,1483"/>
<area shape="rect" id="node34" href="$_eload_8c.html#a220ba0eebf40921c1536740d305103f3" title=" " alt="" coords="577,849,667,875"/>
<area shape="rect" id="node35" href="$spi_8c.html#ad26ad99ad32438be4c880123c08d8ede" title="Returns the Current for a given Value." alt="" coords="764,697,872,723"/>
<area shape="rect" id="node36" href="$spi_8c.html#a8fb1a7434a0afa308a1e334c16867f68" title="Gets the Ampere Seconds consumed." alt="" coords="579,595,665,622"/>
<area shape="rect" id="node37" href="$adc_8h.html#a3b504b59dfbdde96a7a6762da16e1a93" title="Resets the Min/Max values of the Analog Values." alt="" coords="557,1001,687,1027"/>
<area shape="rect" id="node38" href="$spi_8c.html#a8508d5d475a25c17630a31548c739e17" title=" " alt="" coords="570,899,674,926"/>
<area shape="rect" id="node39" href="$lcd_8c.html#a76e163e293ed77d6cecdcadc800d20a7" title="Has to be called once per Second by the surrounding program." alt="" coords="547,1051,697,1078"/>
<area shape="rect" id="node32" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="771,1457,865,1483"/>
<area shape="rect" id="node33" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="749,1507,887,1534"/>
<area shape="rect" id="node46" href="$led_8h.html#afa870201459ed745a0dffe22327ae35f" title="Clears the Overtemp Error Flag and the LED." alt="" coords="751,1659,885,1686"/>
<area shape="rect" id="node47" href="$led_8h.html#aea553a9b3a4abb12927063350a84a44e" title="Sets the SOA Error Flag and the LED." alt="" coords="769,1710,867,1737"/>
<area shape="rect" id="node48" href="$led_8h.html#a26641dea186ec8ea453761150787698f" title="Clears the SOA Error Flag and the LED." alt="" coords="764,1558,872,1585"/>
<area shape="rect" id="node49" href="$spi_8c.html#a6bb86d3005dc9addb4b5695add9e26e4" title="Sets High Current Mode." alt="" coords="747,1609,889,1635"/>
</map>
