Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
SPIADCData_t Struct Reference

## Data Fields
uint16_t | Ihigh
| The Current measured over the 100mR Shunt. Always valid but inaccurate if in low current mode. More...
uint16_t | Ilow
| The Current measured over both Shunts. Invalid if in high Current Range since the 3R3 is shorted by the FET! More...
uint16_t | V
| The Voltage. More...

## Field Documentation

## ◆ V

uint16_t V

The Voltage.

## ◆ Ilow

uint16_t Ilow

The Current measured over both Shunts. Invalid if in high Current Range since the 3R3 is shorted by the FET!

## ◆ Ihigh

uint16_t Ihigh

The Current measured over the 100mR Shunt. Always valid but inaccurate if in low current mode.

The documentation for this struct was generated from the following file:

- spi.h