Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
screenItem_t Struct Reference

Holds the data for a screen item. More...

Collaboration diagram for screenItem_t:
[legend]

## Data Fields
control_t * | control
| E.g. the text of a text field or the enterNumber_t of an input field. More...
uint8_t | retval
| If retval !=0 the screen terminates if the user presses enter. More...

## Detailed Description

Holds the data for a screen item.

This is a control-struct and a return value which is passed if the control is activated.

## Field Documentation

## ◆ control

control_t* control

E.g. the text of a text field or the enterNumber_t of an input field.

## ◆ retval

uint8_t retval

If retval !=0 the screen terminates if the user presses enter.

The documentation for this struct was generated from the following file:

- screen.h