Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
refresh_s Struct Reference

Variables for an auto-refresh-control. More...

## Data Fields
void(* | callback )(uint8_t param)
| Callback function which has to draw the value. More...
uint8_t | param
| Parameter for the callback function. More...
uint8_t | pos
| Position (see also to LCD_LINEn) More...
const controlType_t | type

## Detailed Description

Variables for an auto-refresh-control.

The structure provides a callback function which has to draw the value. It will be called in regular intervals to actualize its content.

## Field Documentation

## ◆ type

const controlType_t type

## ◆ pos

uint8_t pos

Position (see also to LCD_LINEn)

## ◆ callback

void(* callback) (uint8_t param)

Callback function which has to draw the value.

## ◆ param

uint8_t param

Parameter for the callback function.

The documentation for this struct was generated from the following file:

- control.h