<map id="CmdCalibrate" name="CmdCalibrate">
<area shape="rect" id="node1" title="Calibrates the Voltage Sensors." alt="" coords="5,464,105,491"/>
<area shape="rect" id="node2" href="$lcd_8c.html#a3a94c0f44f76db891e66d98966f904e8" title="Clears the LCD and sets Cursor to Home Postion." alt="" coords="755,47,833,74"/>
<area shape="rect" id="node10" href="$lcd_8h.html#afa35e4a61570e2824382729f139fc5be" title="Sets the Brightness of the LCD Backlight." alt="" coords="160,616,289,643"/>
<area shape="rect" id="node11" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="368,464,463,491"/>
<area shape="rect" id="node13" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="571,414,644,440"/>
<area shape="rect" id="node14" href="$usartcmd_8c.html#acd425a5eff84a2a0f365ac31187899b9" title="Receives a Double from the Host." alt="" coords="178,211,271,238"/>
<area shape="rect" id="node15" href="$uart_8h.html#a31900f4f13bc5468a0d1533b6bbbd9ac" title="Asserts RTS to the Host Line, i.e. allows the Host to send Data." alt="" coords="373,262,458,288"/>
<area shape="rect" id="node16" href="$usartcmd_8c.html#aa9fa23bb8ee6b6602434375f28671578" title=" " alt="" coords="383,211,448,238"/>
<area shape="rect" id="node21" href="$spi_8c.html#ab815264416b8e8438b2910c13a010d0f" title="Returns the averaged Value for the Sink Voltage." alt="" coords="545,59,670,86"/>
<area shape="rect" id="node22" href="$spi_8c.html#a6edb30e71a33713abaeda30e56d4bbc2" title="Returns the averaged Value for the Sink Voltage." alt="" coords="558,312,657,339"/>
<area shape="rect" id="node23" href="$spi_8c.html#a80a3e7ab4fc8126893d20222ce18f7ec" title="Returns the averaged Value for the Current." alt="" coords="535,363,680,390"/>
<area shape="rect" id="node26" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="346,768,485,795"/>
<area shape="rect" id="node27" href="$spi_8c.html#ae7d52bffdf79197de02b2064e0615c88" title="Sets the DAC to a certain Current." alt="" coords="173,515,276,542"/>
<area shape="rect" id="node32" href="$delay_8h.html#a32bb3007d169096acb7198ce4d0be5d2" title="Delays for one second. This routine is hard&#45;timed and does not rely on interrupts." alt="" coords="191,667,258,694"/>
<area shape="rect" id="node33" href="$spi_8c.html#acb3eafeb13b87ee2d275605d543c372c" title="Returns the averaged Value for the Current." alt="" coords="153,718,296,744"/>
<area shape="rect" id="node34" href="$spi_8c.html#a9c64a243c6b576aee998df37c8a2f1a1" title="Returns the Life Value for the Current." alt="" coords="156,768,293,795"/>
<area shape="rect" id="node35" href="$adc_8c.html#a2a67d2f19f508cbcad11cec29864f8e8" title="Initializes the On Chip ADC." alt="" coords="191,819,258,846"/>
<area shape="rect" id="node36" href="$uart_8c.html#a2221e416383fe0e3152a0d38b015f306" title=" " alt="" coords="171,870,279,896"/>
<area shape="rect" id="node3" href="$lcd_8c.html#a66337720cc00454cf4d5b4c59d210708" title="Writes a Command&#45;Byte to the Display." alt="" coords="908,91,1013,118"/>
<area shape="rect" id="node4" href="$lcd_8c.html#a8bbe315df5131e3567cf5960938c77e5" title="Waits until the LCD is ready." alt="" coords="1063,66,1138,92"/>
<area shape="rect" id="node8" href="$lcd_8c.html#afd5485a731dca173a51b8270c24404e2" title="Writes a Byte to the Display." alt="" coords="1061,116,1140,143"/>
<area shape="rect" id="node5" href="$lcd_8c.html#af1559a17726b03016098580e375d749e" title=" " alt="" coords="1193,66,1297,92"/>
<area shape="rect" id="node6" href="$lcd_8c.html#a691499026cdf181d4b30b4e42ff2f110" title="Reads a Byte from the LCD." alt="" coords="1351,66,1428,92"/>
<area shape="rect" id="node7" href="$lcd_8c.html#a9a49d41e6b1bc64016ca9adbb8f7ab89" title="Reads a nibble from LCD." alt="" coords="1476,66,1589,92"/>
<area shape="rect" id="node9" href="$lcd_8c.html#a1c6b194d0b91174b01ae5fed203241f5" title="Writes a nibble to the LCD." alt="" coords="1188,116,1303,143"/>
<area shape="rect" id="node12" href="$spi_8c.html#a0e0bc8d4968cb844619c63ac93da1e4e" title="The same as DACSetRaw() but without updating the controls This function has been introduced to allow ..." alt="" coords="547,464,667,491"/>
<area shape="rect" id="node17" href="$lcd_8c.html#a3d6576a7f684f5764f35c778588248cc" title="Sets the Cursor Position." alt="" coords="560,211,655,238"/>
<area shape="rect" id="node19" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="560,110,655,136"/>
<area shape="rect" id="node20" href="$sensors_8c.html#a1bd30a33d99acf39dc419dfcda84a12b" title="Converts a Unreg&#45;Raw ADC Value to Voltage." alt="" coords="556,160,659,187"/>
<area shape="rect" id="node24" href="$spi_8c.html#a79a818f0a054ed66908943ec4bc23099" title="Returns the averaged Value for Load Current." alt="" coords="561,262,653,288"/>
<area shape="rect" id="node18" href="$lcd_8c.html#ab8300df8f51fbc77b8895257c2a8085f" title="Sets the Cursor Position." alt="" coords="755,135,833,162"/>
<area shape="rect" id="node25" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="728,414,860,440"/>
<area shape="rect" id="node28" href="$led_8h.html#afa870201459ed745a0dffe22327ae35f" title="Clears the Overtemp Error Flag and the LED." alt="" coords="348,667,483,694"/>
<area shape="rect" id="node29" href="$led_8h.html#aea553a9b3a4abb12927063350a84a44e" title="Sets the SOA Error Flag and the LED." alt="" coords="366,515,465,542"/>
<area shape="rect" id="node30" href="$led_8h.html#a26641dea186ec8ea453761150787698f" title="Clears the SOA Error Flag and the LED." alt="" coords="361,566,469,592"/>
<area shape="rect" id="node31" href="$spi_8c.html#a6bb86d3005dc9addb4b5695add9e26e4" title="Sets High Current Mode." alt="" coords="344,616,487,643"/>
</map>
