Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
enterNumber_s Struct Reference

parameter set for enterNumber() More...

Collaboration diagram for enterNumber_s:
[legend]

## Data Fields
void(* | changeCallback )(CONTROL_RET action, struct enterNumber_s *control, uint8_t param)
| if not 0, this function is called every time the value changes More...
uint8_t | param
| Is passed to the callback function. More...
uint8_t | pos
| Position (see also to LCD_LINEn) More...
const controlType_t | type
| The type of control. More...
enterNumberVariable_t * | var

## Detailed Description

parameter set for enterNumber()

## Field Documentation

## ◆ type

const controlType_t type

The type of control.

## ◆ pos

uint8_t pos

Position (see also to LCD_LINEn)

## ◆ changeCallback

void(* changeCallback) (CONTROL_RET action, struct enterNumber_s *control, uint8_t param)

if not 0, this function is called every time the value changes

## ◆ param

uint8_t param

Is passed to the callback function.

## ◆ var

enterNumberVariable_t* var

The documentation for this struct was generated from the following file:

- control.h