<map id="IsHighCurrentMode" name="IsHighCurrentMode">
<area shape="rect" id="node1" title="Returns True if High Current Mode is active." alt="" coords="276,107,408,133"/>
<area shape="rect" id="node2" href="$_eload_8c.html#af35578a7ae9d130357ffc9be42ed864d" title="Checks for Time Flags." alt="" coords="140,5,212,32"/>
<area shape="rect" id="node4" href="$spi_8h.html#ae7d52bffdf79197de02b2064e0615c88" title="Sets the DAC to a certain Current." alt="" coords="125,56,227,83"/>
<area shape="rect" id="node5" href="$spi_8h.html#a79a818f0a054ed66908943ec4bc23099" title="Returns the averaged Value for Load Current." alt="" coords="130,107,222,133"/>
<area shape="rect" id="node6" href="$spi_8c.html#a9460c4458d4c26e6186a8ef0dad99edc" title="Calculates the maximum allowable Current This function is designed to be fast enough to be executed f..." alt="" coords="139,157,213,184"/>
<area shape="rect" id="node8" href="$spi_8h.html#a8508d5d475a25c17630a31548c739e17" title=" " alt="" coords="124,208,228,235"/>
<area shape="rect" id="node3" href="$_eload_8h.html#a51bdf9afc51ba51479247b238d86d5fe" title="Process Communication&#45;, Time&#45; and Key&#45;Flags." alt="" coords="5,5,76,32"/>
<area shape="rect" id="node7" href="$spi_8c.html#af9cad97352f5ba9bbd800446131125a6" title="The Interrupt Service Routine for SPI." alt="" coords="19,157,62,184"/>
</map>
