<map id="ISR" name="ISR">
<area shape="rect" id="node1" title="The Interrupt Service Routine for SPI." alt="" coords="5,157,48,184"/>
<area shape="rect" id="node2" href="$led_8h.html#a22e26f80f0daf184920f7be6a9e697dd" title="Switches the red LED on." alt="" coords="113,5,200,32"/>
<area shape="rect" id="node3" href="$spi_8h.html#ae5ca843e5892c4123702493518139346" title="Revoke DAC CS." alt="" coords="96,56,217,83"/>
<area shape="rect" id="node4" href="$spi_8h.html#a18ae1a0c6dc099239795567506f3aeb3" title="Asserts ADC CS." alt="" coords="104,107,209,133"/>
<area shape="rect" id="node5" href="$spi_8h.html#aa5b97073c22aea0499ac0ea88ddb6426" title="Revoke ADC CS." alt="" coords="96,157,217,184"/>
<area shape="rect" id="node6" href="$spi_8h.html#afd62b69041542f83a6b4f3125aec9907" title="Asserts DAC CS." alt="" coords="104,208,209,235"/>
<area shape="rect" id="node7" href="$spi_8c.html#a9460c4458d4c26e6186a8ef0dad99edc" title="Calculates the maximum allowable Current This function is designed to be fast enough to be executed f..." alt="" coords="120,259,193,285"/>
<area shape="rect" id="node10" href="$led_8h.html#aff18b9baea88b2fc57b53ebf407bb6e5" title="Switches the red LED off." alt="" coords="113,309,200,336"/>
<area shape="rect" id="node8" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="265,233,397,260"/>
<area shape="rect" id="node9" href="$led_8h.html#aea553a9b3a4abb12927063350a84a44e" title="Sets the SOA Error Flag and the LED." alt="" coords="282,284,381,311"/>
</map>
