Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
enterNumberVariable_s Struct Reference

## Data Fields
uint8_t | curPos
| cursor position (0=left) More...
char | oldValue [CONTROL_ENTER_NUMBER_MAX_SIZE]
| This value will be restored if the user hits cancel. More...
char * | suffix_s
| This String is displayed after the value. Normally the physical unit (e.g. mA) More...
char | value [CONTROL_ENTER_NUMBER_MAX_SIZE]
| The five digits plus string terminator. More...

## Field Documentation

## ◆ value

char value[CONTROL_ENTER_NUMBER_MAX_SIZE]

The five digits plus string terminator.

## ◆ suffix_s

char* suffix_s

This String is displayed after the value. Normally the physical unit (e.g. mA)

## ◆ oldValue

char oldValue[CONTROL_ENTER_NUMBER_MAX_SIZE]

This value will be restored if the user hits cancel.

## ◆ curPos

uint8_t curPos

cursor position (0=left)

The documentation for this struct was generated from the following file:

- control.h