Electronic Load 1.0 Programmable Constant Current Sink

Variables
Error Flags

## Variables
static const uint8_t | EFLAG_AVG_LOST =64
| New Averages were ready but the New Averages Flag was still set. More...
static const uint8_t | EFLAG_NTC1 =1
| NTC1 (the onboard one) seems non-functional. More...
static const uint8_t | EFLAG_NTC2 =2
| NTC2 (the NTC on the Heat Sink) seems non-functional. More...
static const uint8_t | EFLAG_P12 =8
| +12V Supply out of tolerance More...
static const uint8_t | EFLAG_P5 =4
| +5V Supply out of tolerance More...
static const uint8_t | EFLAG_SOA =16
| Indicates Limits caused by the SOA of the Transistor. Should be somehow displayed! More...
static const uint8_t | EFLAG_TEMP =32
| Heat Sink Overtemp. More...
volatile uint8_t | eflags
| Error Flags. More...

## Detailed Description

Flags indicating an error. They are set when the error condition appears. The Status command displays and clears them.

## Variable Documentation

## ◆ eflags

volatile uint8_t eflags

Error Flags.

## ◆ EFLAG_NTC1

const uint8_t EFLAG_NTC1 =1
| static

NTC1 (the onboard one) seems non-functional.

## ◆ EFLAG_NTC2

const uint8_t EFLAG_NTC2 =2
| static

NTC2 (the NTC on the Heat Sink) seems non-functional.

## ◆ EFLAG_P5

const uint8_t EFLAG_P5 =4
| static

+5V Supply out of tolerance

## ◆ EFLAG_P12

const uint8_t EFLAG_P12 =8
| static

+12V Supply out of tolerance

## ◆ EFLAG_SOA

const uint8_t EFLAG_SOA =16
| static

Indicates Limits caused by the SOA of the Transistor. Should be somehow displayed!

## ◆ EFLAG_TEMP

const uint8_t EFLAG_TEMP =32
| static

Heat Sink Overtemp.

## ◆ EFLAG_AVG_LOST

const uint8_t EFLAG_AVG_LOST =64
| static

New Averages were ready but the New Averages Flag was still set.