Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
volatileConfStruct_t Struct Reference

These values will be calculated by ReadConfig() and/or on-the-fly by measurement. More...

## Data Fields
double | dacHighAdj
| A factor considering RchanP. More...
double | rangeHighLimit
| Above this Current, Eload switches to high current Range. More...
double | rangeLowLimit
| Below this Current, Eload switches to low current Range. More...
double | RchanP
| Calculated Channel Resistance of the FET shorting Rhigh || Rhigh. More...
double | Rhigh
| Value of the Sense Resistor for High Current Range. More...
double | Rlow
| Value of the Sense Resistor for Low Current Range. More...
double | SBa
double | SBb
double | VImax
| Maximum Voltage at IMax. More...

## Detailed Description

These values will be calculated by ReadConfig() and/or on-the-fly by measurement.

All physical units are in SI base units or direct derivates

## Field Documentation

## ◆ Rlow

double Rlow

Value of the Sense Resistor for Low Current Range.

## ◆ Rhigh

double Rhigh

Value of the Sense Resistor for High Current Range.

## ◆ RchanP

double RchanP

Calculated Channel Resistance of the FET shorting Rhigh || Rhigh.

## ◆ dacHighAdj

double dacHighAdj

A factor considering RchanP.

## ◆ rangeHighLimit

double rangeHighLimit

Above this Current, Eload switches to high current Range.

## ◆ rangeLowLimit

double rangeLowLimit

Below this Current, Eload switches to low current Range.

## ◆ VImax

double VImax

Maximum Voltage at IMax.

## ◆ SBa

double SBa

## ◆ SBb

double SBb

The documentation for this struct was generated from the following file:

- config.h