<map id="DoFlags" name="DoFlags">
<area shape="rect" id="node1" title="Process Communication&#45;, Time&#45; and Key&#45;Flags." alt="" coords="5,487,76,513"/>
<area shape="rect" id="node2" href="$_eload_8c.html#aefd1a6765377077adfbbf8ddda17e264" title="Checks for Communication Flags." alt="" coords="282,56,357,83"/>
<area shape="rect" id="node6" href="$_eload_8c.html#af35578a7ae9d130357ffc9be42ed864d" title="Checks for Time Flags." alt="" coords="124,512,196,539"/>
<area shape="rect" id="node3" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="659,157,733,184"/>
<area shape="rect" id="node4" href="$usartcmd_8c.html#aae6978a287d0ea7d42f3e5d1b496ce63" title="Executes one command line." alt="" coords="460,5,571,32"/>
<area shape="rect" id="node5" href="$uart_8h.html#a31900f4f13bc5468a0d1533b6bbbd9ac" title="Asserts RTS to the Host Line, i.e. allows the Host to send Data." alt="" coords="473,56,558,83"/>
<area shape="rect" id="node7" href="$spi_8c.html#a554eba0a42a9236e1069c8478a9142fa" title="Returns the Life Value for the Current." alt="" coords="248,309,391,336"/>
<area shape="rect" id="node8" href="$spi_8c.html#a9c64a243c6b576aee998df37c8a2f1a1" title="Returns the Life Value for the Current." alt="" coords="251,360,388,387"/>
<area shape="rect" id="node9" href="$spi_8c.html#a6f60819b713ab284521b04a3909b532e" title="Returns the Life Value for the Sink Voltage." alt="" coords="257,411,381,437"/>
<area shape="rect" id="node10" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="449,665,581,692"/>
<area shape="rect" id="node11" href="$spi_8c.html#a80a3e7ab4fc8126893d20222ce18f7ec" title="Returns the averaged Value for the Current." alt="" coords="443,804,588,831"/>
<area shape="rect" id="node12" href="$spi_8c.html#acb3eafeb13b87ee2d275605d543c372c" title="Returns the averaged Value for the Current." alt="" coords="444,861,587,888"/>
<area shape="rect" id="node13" href="$spi_8c.html#ab815264416b8e8438b2910c13a010d0f" title="Returns the averaged Value for the Sink Voltage." alt="" coords="257,613,382,640"/>
<area shape="rect" id="node14" href="$sensors_8c.html#a42574109118a2a056f26023de6294ddf" title="Converts a P5&#45;Raw ADC Value to Voltage." alt="" coords="468,563,563,589"/>
<area shape="rect" id="node15" href="$sensors_8c.html#a1bd30a33d99acf39dc419dfcda84a12b" title="Converts a Unreg&#45;Raw ADC Value to Voltage." alt="" coords="268,715,371,741"/>
<area shape="rect" id="node16" href="$sensors_8c.html#a25ac5c6f9d5812eca2a3f84401825dec" title="Converts the ADC&#45;Temp of the Display NTC Value to Celsius This function also calculates the derating ..." alt="" coords="264,563,375,589"/>
<area shape="rect" id="node17" href="$sensors_8c.html#a431ae2d9b1840dcb23cd8a8a08c27a3e" title="Converts the ADC&#45;Temp Value of the Heat Sink NTC to Celsius." alt="" coords="255,968,384,995"/>
<area shape="rect" id="node22" href="$_eload_8c.html#a220ba0eebf40921c1536740d305103f3" title=" " alt="" coords="275,867,364,893"/>
<area shape="rect" id="node23" href="$spi_8c.html#ad26ad99ad32438be4c880123c08d8ede" title="Returns the Current for a given Value." alt="" coords="461,385,569,412"/>
<area shape="rect" id="node24" href="$spi_8c.html#a8fb1a7434a0afa308a1e334c16867f68" title="Gets the Ampere Seconds consumed." alt="" coords="276,259,363,285"/>
<area shape="rect" id="node25" href="$adc_8h.html#a3b504b59dfbdde96a7a6762da16e1a93" title="Resets the Min/Max values of the Analog Values." alt="" coords="255,107,384,133"/>
<area shape="rect" id="node26" href="$spi_8c.html#a8508d5d475a25c17630a31548c739e17" title=" " alt="" coords="267,765,371,792"/>
<area shape="rect" id="node27" href="$lcd_8c.html#a76e163e293ed77d6cecdcadc800d20a7" title="Has to be called once per Second by the surrounding program." alt="" coords="244,208,395,235"/>
<area shape="rect" id="node18" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="468,965,563,992"/>
<area shape="rect" id="node20" href="$led_8h.html#a449e7c96d56eafe4856d89eaafb20583" title="Sets the Overtemp Error Flag and the LED." alt="" coords="453,915,578,941"/>
<area shape="rect" id="node21" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="446,1016,585,1043"/>
<area shape="rect" id="node19" href="$spi_8c.html#a0e0bc8d4968cb844619c63ac93da1e4e" title="The same as DACSetRaw() but without updating the controls This function has been introduced to allow ..." alt="" coords="636,965,756,992"/>
<area shape="rect" id="node28" href="$lcd_8h.html#ade0a120b714ecbdb9a6903ab8cc0287c" title="Gets the current Brightness of the LCD Backlight." alt="" coords="450,259,581,285"/>
<area shape="rect" id="node29" href="$lcd_8h.html#afa35e4a61570e2824382729f139fc5be" title="Sets the Brightness of the LCD Backlight." alt="" coords="451,208,580,235"/>
</map>
