Electronic Load 1.0 Programmable Constant Current Sink

Variables
LED Flashing values

## Variables
static const LED_FLASH_t | LED_BLINK_BEACON = 0b00000001
| short pulse, 200ms on, 1.4s off More...
static const LED_FLASH_t | LED_BLINK_FAST = 0b01010101
| fast blinking, period=0.4s More...
static const LED_FLASH_t | LED_BLINK_NORMAL = 0b00110011
| normal speed blinking, period=0.8s More...
static const LED_FLASH_t | LED_BLINK_OFF = 0b00000000
| always off More...
static const LED_FLASH_t | LED_BLINK_ON = 0b11111111
| always on More...
static const LED_FLASH_t | LED_BLINK_SLOW = 0b00001111
| slow blinking, period=1.6s More...

## Detailed Description

Predefined values for LED flashing

## Variable Documentation

## ◆ LED_BLINK_ON

const LED_FLASH_t LED_BLINK_ON = 0b11111111
| static

always on

## ◆ LED_BLINK_OFF

const LED_FLASH_t LED_BLINK_OFF = 0b00000000
| static

always off

## ◆ LED_BLINK_SLOW

const LED_FLASH_t LED_BLINK_SLOW = 0b00001111
| static

slow blinking, period=1.6s

## ◆ LED_BLINK_NORMAL

const LED_FLASH_t LED_BLINK_NORMAL = 0b00110011
| static

normal speed blinking, period=0.8s

## ◆ LED_BLINK_FAST

const LED_FLASH_t LED_BLINK_FAST = 0b01010101
| static

fast blinking, period=0.4s

## ◆ LED_BLINK_BEACON

const LED_FLASH_t LED_BLINK_BEACON = 0b00000001
| static

short pulse, 200ms on, 1.4s off