Electronic Load 1.0 Programmable Constant Current Sink

Data Fields
commandTable_t Struct Reference

Holds a Table containing all valid Commands and the corresponding Address of the routine handling it. More...

## Data Fields
int8_t(* | adr )(void)
| The address of the program. More...
char * | cmd
| The command string. More...
const char * | helptext
| A short explanation printed with the help command. More...

## Detailed Description

Holds a Table containing all valid Commands and the corresponding Address of the routine handling it.

The command string is converted to lower case so case does not matter.

## Field Documentation

## ◆ cmd

char* cmd

The command string.

The string is only evaluated to the length given so you can abbreviate commands. Be sure to use unique abbreviations, though.

## ◆ adr

int8_t(* adr) (void)

The address of the program.

## ◆ helptext

const char* helptext

A short explanation printed with the help command.

If helptext is NULL it will not be listed in the help-command. This helps to implement 'secret' commands that the normal user does not need.

The documentation for this struct was generated from the following file:

- usartcmd.h