<map id="DACSetAmpsByStr" name="DACSetAmpsByStr">
<area shape="rect" id="node1" title="Sets the sink to the value of a string." alt="" coords="5,157,141,184"/>
<area shape="rect" id="node2" href="$spi_8c.html#ae7d52bffdf79197de02b2064e0615c88" title="Sets the DAC to a certain Current." alt="" coords="189,157,292,184"/>
<area shape="rect" id="node3" href="$led_8h.html#afa870201459ed745a0dffe22327ae35f" title="Clears the Overtemp Error Flag and the LED." alt="" coords="344,5,479,32"/>
<area shape="rect" id="node4" href="$led_8h.html#aea553a9b3a4abb12927063350a84a44e" title="Sets the SOA Error Flag and the LED." alt="" coords="362,56,461,83"/>
<area shape="rect" id="node5" href="$led_8h.html#a26641dea186ec8ea453761150787698f" title="Clears the SOA Error Flag and the LED." alt="" coords="357,107,465,133"/>
<area shape="rect" id="node6" href="$spi_8c.html#a6bb86d3005dc9addb4b5695add9e26e4" title="Sets High Current Mode." alt="" coords="340,157,483,184"/>
<area shape="rect" id="node7" href="$spi_8c.html#aedd6d941ec540b8bfcaa011ea11cbbe8" title="Sets Low Current Mode." alt="" coords="342,208,481,235"/>
<area shape="rect" id="node8" href="$spi_8h.html#aa979f2d5b9ebc8e0d60ee3575fb396b8" title="Returns True if High Current Mode is active." alt="" coords="345,259,477,285"/>
<area shape="rect" id="node9" href="$spi_8c.html#a77bb5efc77b2e69919ca98ca241dde46" title="Sets the raw Value of the DAC." alt="" coords="364,309,459,336"/>
<area shape="rect" id="node10" href="$spi_8c.html#a0e0bc8d4968cb844619c63ac93da1e4e" title="The same as DACSetRaw() but without updating the controls This function has been introduced to allow ..." alt="" coords="531,284,651,311"/>
<area shape="rect" id="node11" href="$uart_8c.html#ab820319ed8aea704b9ca0d8b48815a49" title="printf_P for Communication with the Host" alt="" coords="554,335,627,361"/>
</map>
