(footprint "7SegmentLED_SC52-11"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "7-Segment Display, LTS67x0, http://optoelectronics.liteon.com/upload/download/DS30-2001-355/S6760jd.pdf")
	(tags "7Segment LED LTS6760 LTS6780")
	(property "Reference" "REF**"
		(at 0 -10.16 0)
		(layer "F.SilkS")
	)
	(property "Value" "7SegmentLED_SC52-11"
		(at 0 10.16 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "B.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -7.62 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at -5.08 7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole oval
		(at -2.54 7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 2.54 7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 5.08 7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 5.08 -7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 2.54 -7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 0 -7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at -2.54 -7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at -5.08 -7.62)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${RL3D}/sc52-11.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
