(module 7SegmentLED_SC52-11 (layer F.Cu) (tedit 5FC90F53)
  (descr "7-Segment Display, LTS67x0, http://optoelectronics.liteon.com/upload/download/DS30-2001-355/S6760jd.pdf")
  (tags "7Segment LED LTS6760 LTS6780")
  (fp_text reference REF** (at 0 -10.16) (layer F.SilkS))
  (fp_text value 7SegmentLED_SC52-11 (at 0 10.16 180) (layer F.Fab))
  (fp_text user %R (at 0 -7.62) (layer F.Fab))
  (fp_text user %R (at 0 0 90) (layer B.SilkS))
  (pad 2 thru_hole oval (at -2.54 7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole roundrect (at -5.08 7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad 3 thru_hole oval (at 0 7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 2.54 7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 5.08 7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at -2.54 -7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 0 -7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 5.08 -7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 2.54 -7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at -5.08 -7.62) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  (model ${RL3D}/sc52-11.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
