Digital Scale 1.0 Digital Scale

- Main Page
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups
Variables
Flags

## Variables
static const uint8_t | EFLAG_LOBAT =2
| Is set on low Supply Voltage. More...
static const uint8_t | EFLAG_UNCAL =1
| Device has not been calibrated. More...
volatile uint8_t | eFlags
| Error flags. More...
static const uint8_t | TFLAG_SEC =1
| Is set once per Second. More...
volatile uint8_t | tFlags
| Flags set by Time. More...

## Detailed Description

Flags indicating timer events and errors. They are set when the error condition appears.

## Variable Documentation

volatile uint8_t tFlags

Flags set by Time.

volatile uint8_t eFlags

Error flags.

const uint8_t TFLAG_SEC =1
| static

Is set once per Second.

const uint8_t EFLAG_UNCAL =1
| static

Device has not been calibrated.

const uint8_t EFLAG_LOBAT =2
| static

Is set on low Supply Voltage.